# **Invitation For Tender Notice No. 29/2021.**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 01 | Agency | Biman Bangladesh Airlines Ltd. | | | | |
| 02 | Invitation for | Replacement of Old, Rusted & Damaged Gas Pipe Line of BFCC Building. | | | | |
| 03 | Invitation Ref: | 30.34.0000.063.53.112.21 | | | Date: 06-09-2021. | |
| 04 | Tender Document Selling Date | **From 24-10-2021 to 09-11-2021 (During office hours).** | | | | |
| 05 | Tender Closing Date and Time | **Date: 10–11–2021** | Time: 1200 Hrs BST | Note: The procuring entity reserves the right to accept or reject all tenders without assigning any reason thereof. If any unavoidable situation arises during specified date then tender selling/closing/opening date will be shifted to next (working) day without further notice. | | |
| 06 | Tender Opening Date and Time | **Date: 10–11–2021** | Time: 1500 Hrs BST |
| 07 | Selling Address of schedule | a. Manager Finance, Biman Flight Catering Centre, Hazrat Shahjalal International Airport, Kurmitola,Dhaka.b. Manager Cash & Banking, Balaka Bhaban, Biman Bangladesh Airlines Ltd, Dhaka. | | | | |
| 08 | Receiving Tender Document | a. BFCC Main Security Gate, Hazrat Shahjalal International Airport,Kurmitola, Dhaka.b. Biman Balaka Bhaban, Security counter gate (Ground floor), Hazrat Shahjalal International Airport, Kurmitola, Dhaka. | | | | |
| 09 | Price of Tender Schedule | BDT 1,000.00 (One thousand) only per set (Non refundable). | | | | |
| 10 | 1) Location | 2) Tender Security Amount (Tk) | | | | 3) Contract Period |
| BFCC/Hazrat Shahjalal Internatioal Airport, Kurmitola, Dhaka | BDT 30,000.00 (Thirty Thousand) only (Refundable). | | | | One Time |
| 11 | Procuring Entity & Fund | General Manager, BFCC, Hazrat Shahjalal International Airport, Kurmitola, Dhaka & Biman’s own fund. | | | | |
| 12 | Official-Inviting Tender | Dy-General Manager, BFCC, Hazrat Shahjalal International Airport, Kurmitola, Dhaka.Phone: 880-2-8901760-64, Fax: 880-2-8901638 | | | | |
| 13 | Tender schedule and other related information will also be available at Biman website: [www.biman-airlines.com](http://www.biman-airlines.com) for ready reference. | | | | | |

# Dy. General Manager, BFCC.

**`icÎ weÁwß bs-29/2021**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 01 | G‡RÝx | wegvb evsjv‡`k GqvijvBÝ wjt| | | | | |
| 02 | wK Rb¨ Avnevb | weGdwmwmÕi Old, Rusted & Damaged Gas Pipe Line cwieZ©‡bi wbwg‡Ë `icÎ Avnevb| | | | | |
| 03 | `icÎ Avnev‡bi m~Î | 30.34.0000.063.53.112.21 | | | ZvwiL: 06-09-2021 | |
| 04 | `icÎ `wjj weµ‡qi ZvwiL | **24-10-2021 wLªt nB‡Z 09-11-2021 wLªt ch©šÍ (Awdm PjvKvjxb mgq)|** | | | | |
| 05 | `icÎ Mªn‡Yi ZvwiL I mgq | **10-11-2021 wLªt** | mgq:1200 ¯’vbxq mgq | †Kv‡bv KviY `k©v‡bv e¨wZ‡i‡K †h †Kv‡bv/me `icÎ evwZj/MÖnY, `icÎ †Lvjvi ZvwiL cwieZ©b Kivi me©gq ¶gZv weGdwmwm KZ„©c¶ msi¶Y K‡ib| hw` `icÎ †Lvjvi w`b QywU \_v‡K A\_ev Awbevh© †Kv‡bv KviYekZt `icÎ MÖnY/†Lvjv m¤¢e bv nq Zvn‡j cieZx© Kvh©w`em `icÎ `vwLj I †Lvjvi ˆea ZvwiL wnmv‡e MY¨ Kiv n‡e| | | |
| 06 | `icÎ †Lvjvi ZvwiL I mgq | **10-11-2021 wLªt** | mgq:1500 ¯’vbxq mgq |
| 07 | `icÎ `wjj weµqKvix Awdm mg~‡ni bvg I wVKvbv | K) e¨e¯’vcK A\_©, wegvb d¬vBU K¨vUvwis †m›Uvi, nhiZ kvnRvjvj AvšÍR©vwZK wegvbe›`i, Kzwg©‡Uvjv, XvKv|  L) e¨e¯’vcK K¨vk GÛ e¨vswKs, ejvKv feb, wegvb evsjv‡`k GqvijvBÝ wjt XvKv| | | | | |
| 08 | `icÎ MªnYKvix Awdm mg~‡ni bvg I wVKvbv | K) cÖavb †MBU, wegvb d¬vBU K¨vUvwis †m›Uvi, nhiZ kvnRvjvj AvšÍR©vwZK wegvbe›`i, Kzwg©‡Uvjv, XvKv|  L) wegvb ejvKv feb cÖavb †MBU (bxP Zjv), nhiZ kvnRvjvj AvšÍR©vwZK wegvbe›`i, Kzwg©‡Uvjv, XvKv| | | | | |
| 09 | `icÎ `wj‡ji g~j¨ | UvKv 1,000.00 (GK nvRvi) gvÎ cÖwZ †mU (A‡diZ‡hvM¨)| | | | | |
| 10 | **01) Ae¯nvb** | **02) `ic‡Îi Rvgvb‡Zi cwigvY UvKv|** | | | | **03) Pzw³i †gqv`** |
| weGdwmwm/nhiZ kvnRvjvj AvšÍR©vwZK wegvbe›`i, Kzwg©‡Uvjv, XvKv| | UvKv 30,000.00 (wÎk nvRvi) gvÎ (‡diZ‡hvM¨)| | | | | GKKvjxb |
| 11 | `icÎ msMÖnKvix ¯^Z¡vi bvg I Znwej | gnve¨e¯’vcK, weGdwmwm, nhiZ kvnRvjvj AvšÍR©vwZK wegvbe›`i, Kzwg©‡Uvjv, XvKv I wegv‡bi wbR¯^ Znwej| | | | | |
| 12 | Awdwmqvj `icÎ AvnevbKvix | Dc-gnve¨e¯’vcK, weGdwmwm, nhiZ kvnRvjvj AvšÍR©vwZK wegvbe›`i, Kzwg©‡Uvjv, XvKv|  †dvb:880-2-8901760-64, d¨v·: 8901638| | | | | |
| 13 | `icÎ wmwWDjmn Ab¨vb¨ Avbylvw½K mKj Z\_¨vw` Zvr¶wbKfv‡e wegvb I‡qe mvBUt[**www.biman-airlines.com**](http://www.biman-airlines.com)**-**G cvIqv hv‡e| | | | | | |

Dc-gnve¨e¯’vcK, weGdwmwm|

Ref: 30.34.0000.063.2021 Date: 21-10-2021

M/S. .............................................

......................................................

......................................................

# SUB: OTM TENDER SCHEDULE AND OTHER TERMS & CONDITIONS FOR REPLACEMENT OF OLD, RUSTED AND DAMAGED GAS PIPE LINE OF BFCC BUILDING

Selling address of Schedule: Manager, Finance, Biman Flight Catering Centre, HSIA, Dhaka.

# Ref:

a) OTM Tender Notice No. **29/2021** dated 21-10-2021

b) Cost of schedule Tk. **1,000.00** (One thousand) only per set (Non-refundable).

c) Earnest Money Tk. **30,000.00** (Thirty thousand) only (Refundable).

d) Cash receipt no\_\_\_\_\_\_\_\_dated\_\_\_\_\_\_\_\_2021

e) Date & time of dropping the tender: **10-11-2021** up to 1200 hours.

f) Date & time of opening the tender: **10-11-2021** at 1500 hours.

Dear Tenderer

# Enclosed herewith please find the tender schedule along with terms & conditions for OTM TENDER SCHEDULE AND OTHER TERMS & CONDITIONS FOR REPLACEMENT OF OLD, RUSTED AND DAMAGED GAS PIPE LINE OF BFCC BUILDING.

# You may please participate in the tender, if the terms & conditions is acceptable to you.

For-Biman Flight Catering Centre,

Mohammad Ali

Dy. General Manager, BFCC

# Enclosure: As stated.

OTM Tender No 00/2021 Dtd: 00-00-2021

**DATE/TIME DROPPING: 10-11-2021 UP TO 1200 HRS (LT)**

**DATE/TIME OPENING: 10-11-2021 AT 1500 HRS (LT)**

**COST OF SCHEDULE: BDT 1000 (NON REFUNDABLE)**

## **EARNEST MONEY BDT 30,000.00 (Thirty thousand) only (Refundable).**

Approval reference no. 30.34.0000.063.53.112.21 Dated: 06.09.2021

## OTM Tender is hereby invited from M/S. Titas Gas Transmission & Distribution Limited enlisted contractor.

# SUB: OTM TENDER SCHEDULE AND OTHER TERMS & CONDITIONS FOR REPLACEMENT OF OLD, RUSTED AND DAMAGED GAS PIPE LINE OF BFCC BUILDING

Detail specification /schedule is attached in page no. 04-05.

Contd...........P/02

#### Page-02

## The terms & conditions are as follows:

01. Tender shall be submitted in one sealed envelope.

#### 02. Offer of envelope shall contain the following documents (Where applicable).

# i) Original tender schedule with signature and seal of tender in every page.

# ii) ­­Photocopy of valid Trade license of current year.

# iii) Photocopy of VAT registration certificate.

# iv) Photocopy of current income tax certificate with TIN / Photocopy of certificate from the competent authority stating that current income tax return has been submitted quoting TIN number or SIR number.

v) Earnest money of BDT **30,000.00** (Thirty thousand) only (Refundable) in the shape of Pay order/Bank Draft in favour of Biman Flight Catering Centre must be submitted from a scheduled Bank of Bangladesh. The validity of earnest money must be 180 days from the date of opening of the tender.

# vi) Original copy of CR (Cash Money Receipt of Tender schedule purchase).

# vii) Brand and origin must be mentioned in the tender schedule.

# 03. Tender document must be dropped in tender box within the specified time. No tender offer shall be received after the time limit.

# 04. Price is to be quoted by the bidder in their letterhead pad/enclosed price schedule (page 4-5) showing the total price in words & in figure and no amendment will be acceptable.

# 05. All submitted documents must be numerically serial showing total number of sheets. Each sheet must be signed & sealed by the tenderer.

# 06. Overwriting/Erasing on rates quoted may render the tender to be rejected unless properly countersigned by the tenderer. Any use of correcting fluid is not acceptable.

# 07. Experience certificate of similar job from Govt/Semi-Govt/corporate bodies/reputed organization must be submitted.

## Tender shall be rejected if any of the above terms & conditions are not fulfilled.

# 08. BFFC management may give time extension for unavoidable circumstances or logical ground without penalty for supply of items. 0.50% penalty will be imposed per week for late completion of supply/ work without any proper causes.

## 09. Tender in sealed cover will be received in (a) BFCC Main Security Gate, (Land side gate) Hazrat Shahajalal International Airport,Dhaka (b) Balaka Bhaban, Main Security Counter Gate (Ground Floor), Dhaka latest by 1200 hrs (LT) on **10-11-2021.** Offer will be opened on the same day in the Conference room of BFCC, Hazrat Shahjalal International Airport, Dhaka, in presence of the tenderers or his representative(s) if any at 1500 hrs (LT)

# 10. Offer should remain valid for 120 (One Hundred twenty) days from the date of tender opening.

# 11. Only unconditional offer will be accepted.

# 12. Due to unforeseen/unavoidable circumstances revised dates will be the next working days of the tenders closing/opening etc.

# 13. BFCC reserves the right either to increase or decrease the quantities mentioned in the tender schedule and to accept or reject any/ Tender without assigning any reason thereof.

Mohammad Ali

Dy. General Manager, BFCC

Telephone-880-2-8901760-64 Ex-13

Contd.......P/03

Page - 03

## 14. Additional terms & conditions applicable for successful bidder:

1. Work will be completed within 45 (Forty five) days that will be effected from the date of received of work order.
2. Unconditional warranty period shall be 12(Twelve) months from the date of completion of works at BFCC, HSIA, Dhaka
3. NOA will be sent through email and same should be accepted within 5 working days otherwise, it will be treated as not accepted and BFCC have the authority to cancel the offer and forfeit the earnest money and call the 2 nd lowest responsive bidder.
4. 10% of the quoted value require to be submitted by the bidder after receiving the NOA as Performance Security and the same will be refund without any interest after satisfactory completion of warranty period.
5. Upon receiving the performance security, work order will be issued in favour of successful bidder.
6. Income tax or any other tax, VAT, duty etc. that come within the terms and deduction at source will be deducted from the bill and deposit in Govt. fund. A certificate to that effect will be given to the party concerned on written request.
7. Materials to be used must be up to the standard and as per specification of schedule and will be rejected at site if found unacceptable
8. Work will be done as per supplied schedule, enclosed drawing and instruction of Engineer in charge.
9. Contractor has to remove all the rubbish and unused product from BFCC premises within schedule time on his own cost.
10. Work may be suspended several times due to operational activity and VVIP sensitivity.
11. Work may be shifted day to night or vice verse.
12. Contractor must bring all required tools and accessories for completion of the job.
13. Contractor will remain responsible for the safety of materials/jobs until finished work is finally hand over to BFCC authority.
14. The contractor shall be responsible for any kind of accident, failure or any other causes of nonconformities during the work period.
15. Work Completion notification must be submitted after complete the job.
16. Gas flow diagram preparing and taking approval from M/S. Titas gas transmission &distribution Ltd. will be done by contractor.
17. Work schedule processing and obtaining approvalfrom M/S. Titas gas transmission & distribution Ltd. will be done by contractor.
18. All other required official process of M/S. Titas gas transmission & distribution Ltd. will be done by contractor.
19. Necessary all required accessories for pipe fixing/installation must be supplied by contractor and work will be performed on the roof of bfcc.

Mohammad Ali

Dy. General Manager, BFCC

Telephone-880-2-8901760-64 Ex-13

DECLARATION

#### I/We -------------------------------------------------------M/s. -----------------------------------------------------------------------------------------------------------owner representative hereby declared that I/we have accepted all terms & conditions of tender papers and submitted quotation accordingly.

Contd...........P/04

Page – 04

# Biman Flight Catering Center

# HS International Airport, Dhaka

## OTM Tender Notice No. 29/2021 Dated: 21-10-2021

# Price and delivery schedule of Old, Rusted & Damaged Gas Pipe Line

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Sl No. | Description of Works | Quantity | Unit | Rate in fig. & in Words (Tk) | Total amount (Tk.) |
| 01 | Supply, Fitting & Fixing 3 inch dia MS Gas Pipe lineIncluding all Fitting & Fixing Complete  Pipe Thickness 4mm minimum/api grad B  Pipe must be seamless new pipe. All fittings must be seamless and standard for gas pipe line. All pipe joint with fittings must be as per Titas gas ltd. specification and standard and direction of the engineer in charge including flange and valve | 265 | Rft |  |  |
| 02 | Supply, Fitting & Fixing 2 inch dia MS Gas Pipe line Including all Fitting & Fixing Complete  Pipe Thickness 4mm minimum/api grad B  Pipe must be seamless new pipe. All fittings must be seamless and standard for gas pipe line. All pipe joint with fittings must be as per Titas gas ltd. specification and standard and direction of the engineer in charge including flange and valve | 160 | Rft |  |  |
| 03 | Supply, Fitting & Fixing 1 inch dia MS Gas Pipe line Including all Fitting & Fixing Complete  Pipe Thickness 3mm minimum/api grad B  Pipe must be seamless new pipe. All fittings must be seamless and standard for gas pipe line. All pipe joint with fittings must be as per Titas gas ltd. specification and standard and direction of the engineer in charge including flange and valve | 125 | Rft |  |  |

SIGNATURE OF THE BIDDER WITH OFFICIAL SEAL

Contd.......P/05

Page 05

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Sl No. | Description of Works | Quantity | Unit | Rate in fig. & in Words | Total amount (Tk.) |
| 04 | Supply, Fitting & Fixing 3 inch dia MS Gas Shutoff Valve (Foreign)  Valve must be rustproof best quality Flange type natural gas shutoff valve and Titas gas standard.  Brand:  Origin: | 03 | Nos |  |  |
| 05 | Supply, Fitting & Fixing 2 inch dia Gas Shutoff Valve (Foreign)  Valve must be rustproof best quality Titas gas standard  Brand:  Origin: | 03 | Nos |  |  |
| 06 | Supply, Fitting & Fixing 1 inch dia Gas Shutoff Ball Valve (Foreign)  Valve must be rustproof best quality Titas gas standard1 inch dia  Brand:  Origin: | 18 | Nos |  |  |
| 07 | Supply, Fitting & Fixing 1 inch diaGas Regulator (Foreign)  Regulator must be rustproof best quality Titas gas standard and mbar adjustment  Brand:  Origin: | 03 | Nos |  |  |

SIGNATURE OF THE BIDDER WITH OFFICIAL SEAL